| ManualsContentsPreviousNext |

# Adjusting Printing Position

You can adjust the printing position for trays 2-4.

1. Press the [User Tools/Counter] key.

2. Press [Maintenance].

3. Press [Adjust Print Position].

4. Press [Print Test Sheet].

5. Press [Start Printing].

6. Confirm the position of the image on the test sheet, and then adjust the registration value.

   Use this sheet to confirm the current print position.

7. Select the tray you want to adjust.

8. Press [] or [] to specify the vertical position.

   You can specify the printing position between -5.0 mm to 5.0 mm in increments of 0.1 mm.

9. Press [] or [] to specify the horizontal position.

10. Press [OK].

11. Print the test sheet to confirm the adjustment result.

12. Press [Exit] three times.