| ManualsContentsPreviousNext |

# domainname

Use the "domainname" command to display or configure the domain name settings.

You can configure the Ethernet interface or IEEE 802.11 interface.

View settings

The following command displays the current domain name:

`msh> domainname`

Interface domain configuration

`msh> domainname "interface_name"`

Setting the Domain Name

`msh> domainname "interface_name" name "domain name"`

- A domain name can be entered using up to 63 alphanumeric characters.

- The Ethernet interface and IEEE 802.11 interface will have the same domain name.

- wlan can be specified only when the IEEE 802.11 interface is installed.

Interface | Interface set
--- | ---
ether | Ethernet interface
wlan | IEEE 802.11 interface

Deleting the Domain Name

`msh> domainname "interface_name" clear name`