| ManualsContentsPreviousNext |

# Checking Transmission Using LAN-Fax Driver

From Web Image Monitor, you can check information about files sent using LAN-Fax Driver.

For the maximum number of transmission results you can check, see “Maximum Values”.

- The job history may differ from the machine's transmission results. In that case, refer to the machine's transmission results.

- See the Web Image Monitor's Help for details.

- Maximum Values