| ManualsContentsPreviousNext |

# Size Magnification

This function calculates a reproduction ratio based on the lengths of the original and copy.

Measure and specify the lengths of the original and copy by comparing “A” with “a”.

1. Press [Reduce / Enlarge].

2. Press [Size Magnification].

3. Enter the length of the original with the number keys, and then press [].

   You can enter sizes between 1 to 999 mm (0.1 to 99.9 inches) in increments of 1 mm (0.1 inches).

4. Enter the length of the copy with the number keys, and then press [].

5. Press [OK] twice.

- To change the value you entered, press the key you want to change, and then enter a new value.

- If the calculated ratio is over the maximum or under the minimum ratio, it is automatically adjusted to within available range. However, with some ratios, parts of the image might not be copied or margins will appear on copies.

- The machine selects reproduction ratios of between 25 and 400%. However, if the originals are placed in the ADF, the maximum reproduction ratio is 200%. To copy originals at a reproduction ratio above 200%, you must place them on the exposure glass.