| ManualsContentsPreviousNext |

# Enabling WSD using Web Image Monitor

To use this machine as a WSD scanner, you must first configure the following settings using Web Image Monitor on a client computer:

- Settings to enable WSD (Push Type)

  - WSD protocol (default setting: [Active])

    Click [Configuration], click [IPv4] under [Network], and then enable [WSD (Scanner)].

  - [Display WSD Destination List] (default setting: [Do not Display])

    Click [Configuration], click [Initial Settings] under [Scanner], and then set [Display WSD Destination List] to [Display].

- Settings to enable WSD (Pull Type)

  - WSD protocol (default setting: [Active])

    Click [Configuration], click [IPv4] under [Network], and then enable [WSD (Scanner)].

  - [Prohibit WSD Scan Command] (default setting: [Prohibit])

    Click [Configuration], click [Initial Settings] under [Scanner], and then set [Prohibit WSD Scan Command] to [Do not Prohibit].

Use the following procedure to enable both WSD (Push Type) and WSD (Pull Type).

1. On the [Start] menu, click [Network].

2. Double-click the icon for this machine.

3. Click [Login].

   The Web Image Monitor login page appears.

4. Enter your login user name and password in the [Login User Name] and [Login Password] boxes respectively, and then click [Login].

   Consult your administrator if you require a login user name and password.

5. On the menu in the left frame, click [Configuration].

6. Under [Scanner], click [Initial Settings].

   The [Initial Settings] page appears.

7. Set [Display WSD Destination List] to [Display].

8. Set [Prohibit WSD Scan Command] to [Do not Prohibit].

9. Click [OK].

- For details about displaying Web Image Monitor, see "Monitoring and Configuring the Machine", Network and System Settings Reference. For details about using Web Image Monitor, see Web Image Monitor Help.