ManualsContentsPreviousNext
Settings

# Ethernet

This section lists the settings required for using Internet Fax with an Ethernet connection.

For details about how to specify the settings, see "Interface Settings" and "File Transfer".

Menu | User Tool | Setting Requirements
--- | --- | ---
Interface Settings/Network | Machine IPv4 Address | Necessary
Interface Settings/Network | IPv4 Gateway Address | Necessary
Interface Settings/Network | Machine IPv6 Address | As required
Interface Settings/Network | IPv6 Gateway Address | As required
Interface Settings/Network | IPv6 Stateless Address Autoconfiguration | As required
Interface Settings/Network | DNS Configuration | As required
Interface Settings/Network | DDNS Configuration | As required
Interface Settings/Network | IPsec | As required
Interface Settings/Network | Domain Name | As required
Interface Settings/Network | WINS Configuration | As required
Interface Settings/Network | Effective Protocol | Necessary
Interface Settings/Network | Ethernet Speed | As required
Interface Settings/Network | LAN Type | Necessary
Interface Settings/Network | Permit SNMPv3 Communication | As required
Interface Settings/Network | Permit SSL / TLS Communication | As required
Interface Settings/Network | Host Name | As required
Interface Settings/Network | IEEE 802.1X Authentication for Ethernet | As required
File Transfer | SMTP Server | Necessary
File Transfer | SMTP Authentication | As required
File Transfer | POP before SMTP | As required
File Transfer | Reception Protocol | As required
File Transfer | POP3 / IMAP4 Settings | As required
File Transfer | Administrator's E-mail Address | As required
File Transfer | E-mail Communication Port | Necessary
File Transfer | E-mail Reception Interval | As required
File Transfer | Max. Reception E-mail Size | As required
File Transfer | E-mail Storage in Server | As required
File Transfer | Program / Change / Delete E-mail Message | As required
File Transfer | Fax E-mail Account | Necessary

- For the Effective Protocol setting, check that the protocol you want to use is set to [Active].

- [LAN Type] is displayed when the wireless LAN board is installed. If both Ethernet and wireless LAN are connected, the selected interface takes precedence.

- SMTP Server and Fax E-mail Account must be specified in order to send Internet Fax.

- When POP before SMTP is set to [On], you must also make settings for Reception Protocol and POP3 / IMAP4 Settings.

- When SMTP Authentication is set to [On], you must also make setting for Administrator's E-mail Address.

- POP3 / IMAP4 Settings, E-mail Communication Port, and Fax E-mail Account must be specified in order to receive Internet Fax.

- When setting POP before SMTP to [On], check POP3 port number in E-mail Communication Port.

- Interface Settings

- File Transfer