| ManualsContentsPreviousNext |

# Ethernet

This section lists the settings required for using the Document Server function with an Ethernet connection.

For details about how to specify the settings, see "Interface Settings".

Menu | User Tool | Setting Requirements
--- | --- | ---
Interface Settings/Network | Machine IPv4 Address | Necessary
Interface Settings/Network | IPv4 Gateway Address | As required
Interface Settings/Network | Machine IPv6 Address | As required
Interface Settings/Network | IPv6 Gateway Address | As required
Interface Settings/Network | IPv6 Stateless Address Autoconfiguration | As required
Interface Settings/Network | DNS Configuration | As required
Interface Settings/Network | DDNS Configuration | As required
Interface Settings/Network | IPsec | As required
Interface Settings/Network | Domain Name | As required
Interface Settings/Network | WINS Configuration | As required
Interface Settings/Network | Effective Protocol | Necessary
Interface Settings/Network | Ethernet Speed | As required
Interface Settings/Network | LAN Type | Necessary
Interface Settings/Network | Permit SNMPv3 Communication | As required
Interface Settings/Network | Permit SSL / TLS Communication | As required
Interface Settings/Network | Host Name | As required
Interface Settings/Network | IEEE 802.1X Authentication for Ethernet | As required

- For the Effective Protocol setting, check that the protocol you want to use is set to [Active].

- [LAN Type] is displayed when the wireless LAN board is installed.

- When both Ethernet and wireless LAN are connected, the selected interface takes precedence.

- Interface Settings