ManualsContentsPreviousNext
Settings

# Setting a port number

When using IP address and port number

To send to an IP-Fax destination, depending on the receiver's network configuration, you might have to specify the IPv4 address and port number of the receiving machine. For example, if the receiver's IPv4 address is “192.168.1.10” and the port number is “2100”, specify “192.168.1.10:2100”. Similarly, if the receiver's IPv6 address is “fe80::0123:4567:89ab:cdef” and the port number is “2200”, specify “[fe80::0123:4567:89ab:cdef]:2200”. Ask your network administrator for details.

When using host name and port number

When you specify a host name, depending on the receiver's network configuration, you may need to specify the host name and port number of the receiving machine. For example, if the receiver's host name is “IPFAX1” and the port number is “2100”, specify “IPFAX1:2100”. Ask the network administrator for details.