ManualsContentsPreviousNext
Settings

# Interrupt Copy

Use this function if you want to interrupt a long copy job to make urgently needed copies.

- You cannot use the Interrupt Copy function when fax originals are being scanned or the scanner function is being used.

- You cannot use the Staple function with this function if another copy job is already using the Staple function.

Press the [Interrupt] key.

The interrupt key indicator lights. The machine stops scanning.

Remove the originals that were being copied.

Place the originals you want to copy.

Press the [Start] key.

The machine starts making copies.

When copying is complete, remove the originals and copies.

Press the [Interrupt] key again.

The interrupt key indicator goes off.

Replace the originals that you were copying, and then press the [Start] key.

Following the instructions on the display.

- The previous copy job settings are restored. Simply press the [Start] key to continue copying from where it left off.