| ManualsContentsPreviousNext |

# Connecting the Machine to a Telephone Line and Telephone

This section describes how to connect the machine to the telephone lines.

- Make sure the connector is the correct type before you start.

To connect the machine to a telephone line, use a snap-in modular type connector.

1. Connect a telephone line cord to the G3 interface unit connector (LINE).

2. If using an external telephone, connect the telephone to the external telephone connector (TEL).

- After connecting the machine to the telephone line, specify the country code, telephone line type, and fax information. For details, see “Initial Settings”, Facsimile Reference.

- If you are using an external telephone, specify the reception mode. For details about specifying the reception mode, “Reception Settings”, Facsimile Reference.

- If your telephone has functions that are not compatible with this machine, those functions cannot be used.