ManualsContentsPreviousNext
Settings

# Mixing Scan Settings for a Multiple Page Original

When sending an original of several pages, you can select a different scan setting for each page.

It is recommended that originals be placed on the exposure glass when mixing scan settings for a multiple page original.

- If you are using the ADF, do not change the “Resolution” setting while originals are being scanned.

When placing originals on the exposure glass

1. Check which pages you want to scan with different settings.

2. Remove the previous page and place the next page that you checked on the exposure glass.

3. Make the scan settings.

   You have about 60 seconds (10 seconds for Immediate Transmission) to make the scan settings. The time remaining is shown on the display.

   Adjust the settings for each page before you press the [Start] key.

When placing originals in the ADF

1. Check which pages you want to scan with different settings.

2. Make the scan settings before the page you want to change the settings for starts being scanned.

   Depending on what time the scan settings are adjusted, the settings may not be reflected in the resulting operation.