| ManualsContentsPreviousNext |

# Specifying a Destination

This section explains how to specify a destination.

Fax numbers, IP-Fax destinations, Internet Fax destinations, e-mail destinations, and folder destinations can be specified.

- The display shows the percentage of free memory space for storing originals. Since destinations are programmed in separate memory, dialing fax numbers using the number keys does not change the percentage on the display.

Related topics

Sending over a Fax Line (Fax Destinations)
Sending by IP-Fax (IP-Fax Destinations)
Sending by Internet Fax (Internet Fax Destinations)
Sending an E-mail (E-mail Destinations)
Sending to Folder Destinations (Folder Destinations)
Using the Address Book to Specify Destinations
Specifying Group Destinations
International TX Mode
Selecting Destinations from Recent Destinations
Preventing Transmission to the Wrong Destination