ManualsContents
SettingsHelp

# Specifying a Fax Number by Entering It Manually

Previous Next

This section explains how to enter a fax number using the number keys.

Make sure that [Fax] is selected.

Enter the fax number using the number keys.

If you make a mistake, press the [Clear] key, and then enter again.

To add a destination, press [Add], and then specify the next destination.

If you use the Address Book to specify the next destination, press the destination key.

- You can insert pauses and tones in a fax number. For details, see Entering a pause or Entering a tone.

- If the optional extra G3 interface unit is installed, select the line you want to use before pressing the [Start] key. For details about selecting a line, see Changing the Line Port.

- For the maximum number of digits that can be included in a destination, see Maximum Values.

Related topics

Entering a pause
Entering a tone
PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search