ManualsContents
SettingsHelp

# Configuring the Network Interface Board

Previous Next

Use the following command to display network interface board settings:

- telnet : Use the "show" command.

The following items may not be displayed depending on the implementation of applications and optional items.

Common

The following items are displayed: ("Up" indicates enabled; "Down" indicates disabled):.

- Mode

- Protocol Up/Down*1

  IPv4, IPv6, IPsec, NetWare, SMB, PictBridge

- Device Up/Down*1

  Parallel, USB, Bluetooth

- Ethernet interface

- Syslog priority

- NVRAM version

- Device name

- Comment

- Location

- Contact

- Soft switch

*1 Parallel, USB and PictBridge are not displayed when the Network Administrator account is logged in to the machine. Only Parallel, USB and PictBridge are displayed when the Machine Administrator account is logged in to the machine.

TCP/IP

The following items are displayed: ("Up" indicates enabled; "Down", indicates disabled):.

- Mode (IPv4)

- Mode (IPv6)

  ftp*1, lpr*1, rsh*1, diprint*1, web, http*1, ftpc, snmp, ipp*1, autonet, Bonjour*1, ssl*1, nrs, rfu*1, nbt, ssdp, ssh, sftp*1, WSD (Device)*1 *2, WSD (Printer), WSD (Scanner), rhpp*1, llmnr, llmnrc

- IPv4

  DHCP, Address, Netmask, Broadcast, Gateway

- IPv6

  Stateless, Manual, Gateway, DHCPv6, Mode, DUID, IAID, Encode RFC, Previous Lease Address

- IPsec

  Manual Mode, Excluded Protocol*3 (https, dns, dhcp, wins)

- EncapType*4

- Host name

- DNS Domain

- Access Control

  IPv4: Access Entry [1]-[5]

  IPv6: Access Entry*5 [1]-[5]

- SNTP Server*6 *7

- Time Zone*6

- SNTP Server polling time*6

- SYSLOG server

- Home page URL1

- Home page link name1

- Home page URL2

- Home page link name2

- Help page URL

- RHPP Port

- RHPP timeout

- HTTP Keep –Alive

- HTTP Keep -Alive timeout

*1 Either of the following items is displayed:

- IPv4:Up, IPv6:Up => Up (IPv4/IPv6)

- IPv4:Up, IPv6:Down => Up (IPv4)

- IPv4:Down, IPv6:Up => Up (IPv6)

- IPv4:Down, IPv6:Down => Down

*2 If both IPv4 and IPv6 are enabled, "Up (IPv4/IPv6)" is displayed for " WSD(Device):". However, it works only with IPv4, not with IPv6. If IPv4 and IPv6 under "Protocol Up/Down" in "Common" are Down and Up respectively, "Up (IPv4/IPv6)" may be displayed for "WSD(Device):". However, it does not work with IPv6.

*3 On/Off will be displayed for each protocol that is excluded.

*4 Either of the following items is displayed. IPX is displayed only if an optional NetWare unit is installed:

- IPv4:Up, IPv6:Up, IPX:Up => IPv4 IPv6 IPX

- IPv4:Up, IPv6:Up, IPX:Down => IPv4 IPv6

- IPv4:Up, IPv6:Down, IPX:Up => IPv4 IPX

- IPv4:Down,IPv6:Up, IPX:Up => IPv6 IPX

- IPv4:Up, IPv6:Down, IPX:Down => IPv4

- IPv4:Down, IPv6:Up , IPX:Down => IPv6

- IPv4:Down, IPv6:Down, IPX:Up => IPX

*5 If IPv6 addresses that are excluded from Printer Job Authentication are specified by range, the starting and ending addresses are displayed for "AuthFree Entry". If such IPv6 addresses are specified by mask length, the base IP address and mask are displayed for "AuthFree Entry".

*6 Items related to the time server are displayed only when the Machine Administrator account is logged in to the machine. In this case, the items under "TCP/IP:" are also displayed.

*7 Either the NTP address or NTP server name is displayed for "SNTP Server".

NetWare

The following items are displayed:

- EncapType

- RPRINTER number

- Print server name

- File server name

- Context name

- Switch

  Mode, NDS/Bindery, Packet negotiation, Login Mode

- Print job timeout

- Protocol

- SAP interval time

- NDS Tree Name

- Transfer Protocol

SMB

The following items are displayed:

- Switch

  Mode, Direct print, Notification

- Workgroup name

- Computer name

- Comment

- Share name [1]

- Protocol

- Client port

- Client auth level

- Client WSD browse

Wireless LAN

The following items are displayed:

- Host name

- Communication Mode

- SSID

- Channel

- Security

- WEP Authentication

- WEP Encryption key number

- WEP Encryption keys [1]-[4]

- WPA Encryption

- WPA Authentication

- Pre-Shared Key

- User name

- Domain name

- EAP Type

- Password

- Phase 2 user name

- Phase 2 Method TTLS

- Phase 2 Method PEAP

- Server cert.

- Intermediate CA

- Server ID

- Sub domain

- Mic check

Ethernet

The following item is displayed:

- 802.1X Authentication

DNS

The following items are displayed:

- IPv4

  Server [1]-[3], Selected IPv4 DNS Server

- IPv6

  Server [1]-[3], Selected IPv6 Dns Server

- Resolver Protocol*1

*1 This item is displayed only when both IPv4 and IPv6 are enabled.

Domain name

The following items are displayed:

- ether

- wlan

DDNS

The following items are displayed:

- ether

- wlan

WINS

The following items are displayed:

- ether

  Primary WINS, Secondary WINS

- wlan

  Primary WINS, Secondary WINS

Bluetooth

The following item is displayed:

- Bluetooth mode

SSDP

The following items are displayed:

- UUID

- Profile

- TTL

UPnP

The following item is displayed:

- URL

Bonjour

The following items are displayed:

- Computer Name (cname)

- Local Hostname (ether)

- Local Hostname (wlan)

- Location

- Priority (diprint)

- Priority (lpr)

- Priority (ipp)

- IP TTL

- LinkLocal Route for Multi I/F

- IPP Port

SNMP

The following items are displayed:

- SNMPv1v2

- SNMPv3

- protocol*1

- v1Trap

- v2Trap

- v3Trap

- SNMPv1v2 Remote Setting

- SNMPv3 Privacy

*1 Either of the following items is displayed. IPX is displayed only if an optional NetWare unit is installed:

- IPv4:Up, IPv6:Up, IPX:Up => IPv4 IPv6 IPX

- IPv4:Up, IPv6:Up, IPX:Down => IPv4 IPv6

- IPv4:Up, IPv6:Down, IPX:Up => IPv4 IPX

- IPv4:Down,IPv6:Up, IPX:Up => IPv6 IPX

- IPv4:Up, IPv6:Down, IPX:Down => IPv4

- IPv4:Down, IPv6:Up , IPX:Down => IPv6

- IPv4:Down, IPv6:Down, IPX:Up => IPX

ssh

The following items are displayed:

- Compression

- Port

- TimeOut

- LoginTimeOut

AuthFree*1

The following items are displayed:

- IPv4

  AuthFree Entry [1]-[5]

- IPv6

  AuthFree Entry*2 [1]-[5]

- Parallel

- USB

*1 This item is displayed only when the following three conditions are met: user authentication is activated, Printer Job Authentication is set to "Simple (Limitation)", and also when the Machine Administrator account is logged in to the machine.

*2 If IPv6 addresses that are excluded from Printer Job Authentication are specified by range, the starting and ending addresses are displayed for "AuthFree Entry". If such IPv6 addresses are specified by mask length, the base IP address and mask are displayed for "AuthFree Entry".

LPR

The following items are displayed:

- lprm check host

- lpr prnerrchk

Certificate

The following item is displayed:

- Verification

WS-MFP

The following items are displayed:

- Network Device Name

- Comments

- Location

- Presentation URL

- WSD (Device) TCP Port

- WSD (Printer) TCP Port

- WSD (Printer) Job Timeout

- WSD (Scanner) TCP Port

- SSL /TLS

- MetadataVersion

- UUID

IEEE 802.1X

The following items are displayed:

- User name

- Domain name

- EAP Type

- Password

- Phase 2 user name

- Phase 2 Method TTLS

- Phase 2 Method PEAP

- Server cert

- Intermediate CA

- Server ID

- Sub domain

Shell mode

"User mode" is displayed.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search