ManualsContents
SettingsHelp

# authfree

Previous Next

Use the "authfree" command to view and configure authfree parameters.

View settings

The following command displays the current authfree settings:

`msh> authfree`

IPv4/IPv6 configuration display

`msh> authfree "ID"`

IPv4 address configuration display

`msh> authfree "ID" range`

IPv6 address configuration display

`msh> authfree "ID" range6`

IPv6 address mask configuration display

`msh> authfree "ID" mask6`

IPv4 address configuration

`msh> authfree "ID" range_addr1 range_addr2`

IPv6 address configuration

`msh> authfree "ID" range6_addr1 range6_addr2`

IPv6 address mask configuration

`msh> authfree "ID" mask6_addr1 masklen`

Parallel/USB configuration

`msh> authfree [parallel | usb] [on|off]`

- To enable authfree, set to [on]. To disable authfree, set to [off]. Always specify the interface.

Authentication exclusion control initialization

`msh> authfree flush`

- Authentication exclusion control is displayed only when print job authentication exclusion is set.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search