ManualsContents
SettingsHelp

# Recommended Original Sizes and Weights

Previous Next

This section describes the types and weights of originals that can be placed.

Types 1 and 2 (mainly Europe and Asia)

Original location | Original size | Original weight
--- | --- | ---
Exposure glass | Up to A3 |
ARDF (One-sided originals) | A3–A5 11 × 17–81/2 × 11 | 40–128 g/m2 (11–34 lb. Bond)
ARDF (Two-sided originals) | A3–A5 11 × 17–81/2 × 11 | 52–105 g/m2 (14–28 lb. Bond) 11 × 17: 64–105 g/m2 (17–28 lb. Bond)
ARDF (Mixed Sizes mode) | A3, B4 JIS (Japanese Industrial Standard), A4, B5 JIS, 11 × 17, 81/2 × 13, 81/2 × 11 | 52–105 g/m2 (14–28 lb. Bond)

Types 1 and 2 (mainly North America)

Original location | Original size | Original weight
--- | --- | ---
Exposure glass | Up to 11 × 17 |
ARDF (One-sided originals) | 11 × 17–51/2 × 81/2 A3–A4 | 40–128 g/m2 (11–34 lb. Bond)
ARDF (Two-sided originals) | 11 × 17–51/2 × 81/2 A3–A4 | 52–105 g/m2 (14–28 lb. Bond) 11 × 17: 64–105 g/m2 (17–28 lb. Bond)
ARDF (Mixed Sizes mode) | 11 × 17, 81/2 × 14, 81/2 × 11, 10 × 14, 71/4 × 101/2, A3, A4 | 52–105 g/m2 (14–28 lb. Bond)

Types 3 and 4 (mainly Europe and Asia)

Original location | Original size | Original weight
--- | --- | ---
Exposure glass | Up to A3 |
ADF (One-sided originals) | A3–B6 JIS 11 × 17–81/2 × 11 | 40–128 g/m2 (11–34 lb. Bond)
ADF (Two-sided originals) | A3–A5 11 × 17–81/2 × 11 | 52–128 g/m2 (14–34 lb. Bond)
ADF (Mixed Sizes mode) | A3, B4 JIS, A4, B5 JIS, 11 × 17, 81/2 × 13, 81/2 × 11 | 52–81 g/m2 (14–20 lb. Bond)

Type 3 and 4 (mainly North America)

Original location | Original size | Original weight
--- | --- | ---
Exposure glass | Up to 11 × 17 |
ADF (One-sided originals) | 11 × 17–51/2 × 81/2 A3–A4 | 40–128 g/m2 (11–34 lb. Bond)
ADF (Two-sided originals) | 11 × 17–51/2 × 81/2 A3–A4 | 52–128 g/m2 (14–34 lb. Bond)
ADF (Mixed Sizes mode) | 11 × 17, 81/2 × 14, 81/2 × 11, 10 × 14, 71/4 × 101/2, A3, A4 | 52–81 g/m2 (14–20 lb. Bond)

- With types 1 and 2, about 50 originals can be loaded in the ARDF. Specifications can vary depending on the type and condition of the paper.

- With types 3 and 4, about 100 originals can be loaded in the ADF. Specifications can vary depending on the type and condition of the paper.

Related topics

Maximum Scan Area
Missing Image Area
PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search