ManualsContents
SettingsHelp

# Communication Failure Report

Previous Next

This report is printed when a document could not be successfully transmitted with Memory Transmission.

This report is only printed if the Communication Result Report is turned off and a document could not be successfully transmitted with Memory Transmission. If the machine is set up to print a Communication Result Report, this report is not printed.

You can select whether the Communication Failure Report is automatically printed using the User Parameter (switch 04, bit 1) in the Facsimile Features menu. See Parameter Settings.

- The Pg(s) column gives the total number of pages. The Page Not Sent column gives the number of pages that could not be sent successfully.

- "Unprogrammed" indicates that the document could not be sent because the forwarding destination is not programmed.

- "--" indicates that the e-mail or Internet Fax document was sent to the mail server programmed in this machine. (However, this does not mean the e-mail was delivered.)

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search