ManualsContents
SettingsHelp

# SUB Code Transfer Report

Previous Next

You can check the results of transmission to Receiving Stations. The machine prints this report when it has finished transmitting to Receiving Stations.

You can select whether the SUB Code Transfer Report be automatically printed using the User Parameter (switch 04, bit 1) in the Facsimile Features menu. See Parameter Settings.

- "Unprogrammed" indicates the document could not be sent because the end receiver is not programmed.

- "--" indicates that the e-mail or Internet Fax document was sent to the mail server programmed in this machine.

- For the maximum number of destinations you can register in a group, see Maximum Values.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search