ManualsContents
SettingsHelp

# Replacing the Stamp Cartridge of Types 3 and 4

Previous Next

Open the ARDF cover.

Raise lever P2, and then pull open cover P2.

Push on the area of cover P3 marked "PUSH", and then open the cover P3.

Pull out the old stamp cartridge.

Insert the new stamp cartridge.

Push in the cartridge until the metal parts are no longer visible.

Close cover P3, P2, and the ARDF cover.

- The one-pass duplex scanning ADF does not support the transmission stamp function.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search