ManualsContents
SettingsHelp

# domainname

Previous Next

Use the "domainname" command to display or configure the domain name settings.

You can configure the Ethernet interface or IEEE 802.11 interface.

View settings

The following command displays the current domain name:

`msh> domainname`

Interface domain configuration

`msh> domainname "interface_name"`

Setting the Domain Name

`msh> domainname "interface_name" name "domain name"`

- A domain name can be entered using up to 63 alphanumeric characters.

- The Ethernet interface and IEEE 802.11 interface will have the same domain name.

- wlan can be specified only when the IEEE 802.11 interface is installed.

Interface | Interface set
--- | ---
ether | Ethernet interface
wlan | IEEE 802.11 interface

Deleting the Domain Name

`msh> domainname "interface_name" clear name`

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search