ManualsContents
SettingsHelp

# Non-compatible originals for the Auto Document Feeder

Previous Next

Placing unsuitable originals in the ADF can cause paper misfeeds or black lines, or result in damage to the originals.

Place the following types of originals on the exposure glass instead:

- Stapled or clipped originals

- Perforated or torn originals

- Curled, folded, or creased originals

- Pasted originals

- Originals with adhesive tape, glue or paste stuck to them

- Originals with any kind of coating, such as thermal fax paper, art paper, aluminum foil, carbon paper, or conductive paper

- Originals with perforated lines

- Originals with indexes, tags, or other projecting parts

- Sticky originals such as translucent paper

- Thin or highly flexible originals

- Thick originals such as postcards

- Bound originals such as books

- Transparent originals such as OHP transparencies or translucent paper

- The original might become dirty if it is written with a pencil or a similar tool.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search