ManualsContents
SettingsHelp

# route

Previous Next

Use the "route" command to view and control the routing table.

Specified route information display

`msh> route get "destination"`

- Specify the IPv4 address to destination.

  "0.0.0.0" cannot be specified as the destination address.

Enabling/disabling specified IPv4 destination

`msh> route active {host|net} "destination" {on|off}`

- If you do not specify {host|net}, the host setting is automatically selected.

Adding IPv4 routing table

`msh> route add {host|net} "destination" "gateway"`

- Adds a host or network route to "destination", and a gateway address to "gateway" in the table.

- Specify the IPv4 address to destination and gateway.

- If you do not specify {host|net}, the host setting is selected automatically.

- You cannot specify "0.0.0.0" as the destination address.

Setting the Default IPv4 gateway

`msh> route add default {gateway}`

Deleting specified IPv4 destination from routing table

`msh> route delete {host|net} "destination"`

- If you do not specify {host|net}, the host setting is automatically selected.

- IPv4 address of destination can be specified.

Setting IPv6 default gateway

`msh> route add6 default "gateway"`

Adding a specified IPv6 destination to routing table

`msh> route add6 "destination" "prefixlen[1-128]" "gateway"`

- Specify the IPv6 address to destination and gateway.

- If the prefix of the address is between 1 and 127, the network is selected. If the prefix of the address is 128, the host is selected.

- You cannot register a record that has the same destination and prefix as a registered record.

- You cannot register a record that uses "0000:0000:0000:0000:0000:0000:0000:0000" as its destination.

Deleting a specified IPv6 destination from routing table

`msh> route delete6 "destination" "prefixlen"`

- Specify the IPv6 address to destination and gateway.

Displaying information about a specified IPv6 route information

`msh> route get6 "destination"`

- Specify the IPv6 address to destination and gateway.

Enabling/disabling a specified IPv6 destination

`msh> route active6 "destination" "prefixlen[1-128]" {on|off}`

Route initialization

`msh> route flush`

- The maximum number of IPv4 routing tables is 16.

- The maximum number of IPv6 routing tables is 2.

- Set a gateway address when communicating with devices on an external network.

- The same gateway address is shared by all interfaces.

- "Prefixlen" is a number between 1 and 128.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search