ManualsContents
SettingsHelp

# Dos and Don'ts

Previous Next

| Do not place vases, plant pots, cups, toiletries, medicines, small metal objects, or containers holding water or any other liquids, on or close to this machine. Fire or electric shock could result from spillage or if such objects or substances fall inside this machine.

| Do not use flammable sprays or solvents in the vicinity of this machine. Doing so could result in fire or electric shock.

| Do not obstruct the machine's vents. Doing so risks fire caused by overheated internal components.

| Unplug the power cord from the wall outlet before you move the machine. While moving the machine, take care that the power cord is not damaged under the machine. Failing to take these precautions could result in fire or electric shock.

- Before unplugging the power cord or turning off the main power switch, make sure remaining memory space is at 100%, as shown on the screen. See "Turning Off the Main Power", Getting Started.

- After scanning originals continuously, the exposure glass may become warm - this is not a malfunction.

- The area around the ventilation holes might feel warm. This is caused by exhaust air and is not a malfunction.

- If the machine is moved from a cold to a warm place, condensation may form inside it. After moving the machine, do not use it for at least two hours. The machine requires this time to adapt to its new environment.

- Do not turn off the power while the machine is in operation.

- Do not open the covers of the machine when it is in operation. If you do, misfeeds might occur.

- Do not move or tilt the machine when the power is on.

- Do not knock the machine while it is operating (for instance, do not use the machine's surfaces to knock stacks of paper into square).

- Depending on the ambient temperature and humidity, steam may come from the ventilation holes behind the control panel during printing. This is water vapor from the paper, not a sign of malfunction.

- If condensation forms inside the machine as a result of temperature change, the machine may not print properly. To minimize this problem, use the optional anti-condensation heaters.

- The optional anti-humidity heater and the optional anti-condensation heater warm the machine's interior to maintain the proper humidity. The anti-humidity heater continues to warm the machine even if the main power switch is turned off.

Ventilation

When you use this machine in a confined space without good ventilation for a long time or print large quantities, you might detect an odd smell.

This might cause the output paper to also have an odd smell.

When you detect an odd smell, regularly ventilate in order to keep the workplace comfortable.

- Set up the machine so that it does not directly ventilate towards people.

- Ventilation should be more than 30 m3/hr/person.

New machine smell

When a machine is new, it might have a unique smell. This smell will subside in about one week.

When you detect an odd smell, sufficiently ventilate and circulate the air in the room.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search