ManualsContents
SettingsHelp

# Specified Area Repeat

Previous Next

Repeatedly copies a specified portion of the image.

To specify the area you want to repeat, you have to define the value of X1, Y1, X2, and Y2 on the original. Measure the area you want to specify before entering the area settings.

The values are entered as follows:

X1: 0–412 mm (0–16.2 inches)

X2: 20–432 mm (0.8–17.0 inches)

Y1: 0–277 mm (0–10.8 inches)

Y2: 20–297 mm (0.8–11.6 inches)

- You cannot use this function from the ADF.

Measure the length from the base point to the area that you want to copy repeatedly (X1, Y1) and the length and width of the area (X2, Y2).

Press [Edit / Colour].

If [Margin Adj.] is selected, press [Margin Adj.] to cancel it.

Press [Edit Image].

Press [Image Repeat].

Press [Specified Area].

Enter the length of [X1] with number keys, and then press [].

Enter the length of [Y1] with the number keys, and then press [].

Enter the length of [X2] with the number keys, and then press [].

Enter the length of [Y2] with the number keys, and then press [].

Press [OK] twice.

Select the size of copy paper and the reproduction ratio.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search