ManualsContents
SettingsHelp

# Initial Settings

Previous Next

This section describes the user tools in the Initial Settings menu under Facsimile Features.

Parameter Setting

User Parameters allow you to customize various settings to suit your needs.

For details about Parameter Setting, see Parameter Settings.

Parameter Setting: Print List

You can print Parameter Setting list.

Print this list to see the current User Parameter settings. However, not all the parameter settings are printed.

1. Press [Facsimile Features].

2. Press [Initial Settings].

3. Press [Parameter Setting: Print List].

4. Press the [Start] key.

5. Press [Exit].

Program Closed Network Code

Register an ID required for Closed Network communication.

Register a four-digit number using 0 to 9 and A to F (except for 0000 and FFFF).

1. Press [Facsimile Features].

2. Press [Initial Settings].

3. Press [Program Closed Network Code].

4. Enter an ID using the number keys and [A] to [F], and then press [].

5. Press [OK].

6. Press [Exit].

Program Memory Lock ID

Program a Memory Lock ID to be entered before printing documents when the Memory Lock function is activated.

A Memory Lock ID can be any four-digit number, except 0000.

1. Press [Facsimile Features].

2. Press [Initial Settings].

3. Press [Program Memory Lock ID].

4. Enter an ID using the number keys, and then press [].

5. Press [OK].

6. Press [Exit].

For details about printing a file received with Memory Lock, see Printing a File Received with Memory Lock.

Internet Fax Setting

You can select to display the Internet Fax tab or not. When you want to send an Internet Fax, set On to display the tab.

Default: [Off]

Select Dial / Push Phone

Use this function to select a line type when the machine is connected to a G3 analog line.

Dial and Push lines are available for selection.

If the optional extra G3 interface unit is installed, settings for the extra G3 lines appear.

This function is not available in some regions.

Default: [Push Button Phone]

1. Press [Facsimile Features].

2. Press [Initial Settings].

3. Press [Select Dial / Push Phone].

4. Press [Push Button Phone] or [Dial Phone (10PPS)] to select the line, and then press [OK].

5. Press [Exit].

Program Fax Information

Program information to be shown on the display of the other machine and printed as a report. The following information can be programmed.

- Fax Header

- Own Name

- Own Fax Number

For details about how to program Fax Information, see Registering Fax Information.

Enable H.323

Specify whether or not H.323 is used for IP-Fax transmission.

Default: [Off]

Enable SIP

Specify whether or not SIP is used for IP-Fax transmission.

Default: [Off]

H.323 Settings

Set the IPv4 address or host name, and alias telephone number of the gatekeeper.

If you select "On" using the User Parameters, you can use the gatekeeper server. See Parameter Settings (switch 34, bit 0).

You can use numbers, and symbols ("" and "") for registration of the alias telephone number in H.323 Settings. Make sure you enter these characters correctly.

1. Press [Facsimile Features].

2. Press [Initial Settings].

3. Press [H.323 Settings].

4. Configure the settings for the item you want to register.

   Press [Change] for the item you want to register, and then enter the characters.

   To register a gatekeeper address, enter the IPv4 address, and then press [OK].

   To register an alias telephone number, enter the alias telephone number using the number keys, and then press [OK].

5. Press [OK].

6. Press [Exit].

SIP Settings

Set the SIP server's IP address or host name, and SIP user name.

- SIP server's IP address

  You can register either an IPv4 or IPv6 address for the SIP server. You cannot register an IPv4-mapped address.

  A proxy server relays call requests and responses.

  A redirect server processes request destination inquiries.

  A register server registers location information of user agents (which correspond to telephones or facsimiles on public telephone lines) on an IP network.

  Use numbers and periods (".") to enter the correct IPv4 addresses for the SIP server. To obtain the correct IP addresses, consult the administrator.

- SIP user name

  You can use alphanumeric symbols (lower and upper cases) and symbols ("; ", "? ", ": ", "&", "=", "+", "$", ", ", "-", "_", ". ", "! ", "", "", "", "'", "(",") ", "%", "/", "[", "]", and "@") for registration of the SIP User Name. Make sure you enter these characters correctly.

- SIP digest authentication

  You can use alphanumeric symbols (lower and upper cases) and symbols ("!", "$", "%", "&", "'", "(", ")", "*", "+", ",","-", ".", "~", "=", "_") for passwords for SIP digest authentication.

If you select "On" using the User Parameters, you can use the SIP server. See Parameter Settings (switch 34, bit 1).

1. Press [Facsimile Features].

2. Press [Initial Settings].

3. Press [SIP Settings].

4. Configure the settings for the item you want to register.

   Press [Change] for the item you want to register, and then enter the characters.

   To register a proxy server, redirect server or register server, enter the SIP server's IP address, and then press [OK].

   To register a SIP user name, enter the SIP user name, and then press [OK].

5. To use SIP digest authentication, press [Set], and then enter the password.

   Press [Enter], enter the password using up to 128 characters, and then press [OK].

   Re-enter the password after the message Confirm Password appears on the screen, and then press [OK].

6. Press [OK].

7. Press [Exit].

Program / Change / Delete Gateway

Register, change, or delete the gateway used for transmission to IP-Fax.

- Gateway address

  You can register either an IPv4 or IPv6 address for the Gateway. You cannot register an IPv4-mapped address.

- Prefix

  For documents sent using a VoIP gateway to G3 Fax, prefixes can be used. If the first several digits of IP-Fax number and the gateway- specific prefix are identical, documents can be transmitted using the registered digits of the gateway. For example, if both 03 and 04 have been registered as gateway number while 0312345678 is also specified, documents can be transmitted via a VoIP gateway for which 03 is used as a prefix.

  When you wish to use the gateways regardless of the IP-Fax destination numbers, register only the gateway addresses without registering the prefix.

- Program / Change

  1. Press [Facsimile Features].

  2. Press [Initial Settings].

  3. Press [Program / Change / Delete Gateway].

  4. Check that [Program / Change] is selected.

  5. Press a VoIP gateway to register.

     When registering a new VoIP gateway, press [Not Programmed].

  6. Press [Change] for "Prefix".

  7. Enter the Prefix using the number keys, and then press [OK].

     To change the existing prefix, press [Clear], and then enter a new prefix.

  8. Select a protocol.

  9. Press [Change] for "Gateway Address".

  10. Enter the gateway address, and then press [OK].

  11. Press [OK].

  12. Press [Exit] twice.

- Delete

  1. Press [Facsimile Features].

  2. Press [Initial Settings].

  3. Press [Program / Change / Delete Gateway].

  4. Press [Delete], and then select a VoIP gateway to delete.

  5. Press [Delete] on the confirmation message.

  6. Press [Exit] twice.

Menu Protect

You can prevent unauthenticated users from changing the user tools settings.

For details about Menu Protect, see "Security Guide".

E-mail Setting

Set whether or not to use "E-mail" in the fax functions.

Default: [Off]

Folder Setting

Set whether or not to use "Folder" in the fax functions.

Default: [Off]

File Type to Transfer

Specify the file format for files transmitted to e-mail addresses and folders registered as forwarding, destinations of backup file transmission, receivers for Personal Box, or end receivers for Transfer Box.

- TIFF

- PDF

- PDF/A

Default: [TIFF]

Security for E-mail TX Results

Configure whether or not to apply encryption and/or a signature to e-mails transmitted with the E-mail TX Results function.

- Encryption

- Signature

1. Press [Facsimile Features].

2. Press [Initial Settings].

3. Press [Next].

4. Press [Security for E-mail TX Results].

   To encrypt e-mails, press [Encryption].

   To attach a signature to an e-mail, press [Signature].

   After configuring the settings, press [OK].

5. Press [Exit].

For details about the security setting, see Encryption and Signature for Internet Fax/E-mail.

- For details about how to change the Facsimile Features, see "Accessing User Tools", Connecting the Machine/ System Settings.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search