ManualsContents
SettingsHelp

# To set label insertion for IP-Fax destination

Previous Next

When Label Insertion is set to On, the receiver's name and standard messages are printed on the fax message when it is received.

Press [Change] under "Label Insertion".

Press [On].

Press [Change] under "Line 2".

Select a new standard message or press [Manual Entry] to enter a new message.

Enter the new message, and then press [OK].

Press [OK].

Press [Change] under "Line 3".

Select the new standard message, and then press [OK].

Press [OK].

- To change the name, key display and title, see Registering User Information.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search