ManualsContents
SettingsHelp

# Using the LAN-Fax Address Book

Previous Next

You can program and edit destinations in the address list using the Address Book.

To open the Address Book in Windows, on the [Start] menu, point to [All Programs], [LAN-Fax Utilities], and then click [Address Book].

If LAN-Fax Driver has already started up, click [Edit Address Book...].

- When you register fax destinations in the Address Book, for [Line:] under [Fax Number:], the following line types can be selected: G3, G3-2, G3-3, G4, G3 Dir. Auto, G3 PABX Auto, and I-G3. The available line types depend on the machine's configuration. This machine does not support G4. If the machine is connected to an extension telephone line, select "G3 PABX Auto".

Related topics

Reading the LAN-Fax Address Book Help
PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search