ManualsContents
SettingsHelp

# Memory Lock Reception

Previous Next

Specify whether or not to activate Memory Lock reception.

For details about this function, see Printing a File Received with Memory Lock.

To use Memory Lock, pre-register the Memory Lock ID in "Program Memory Lock ID" on the Facsimile Features menu. For details, see Initial Settings.

To store incoming documents from special senders only in Memory Lock, register each sender with "Special Senders to Treat Differently".

This function cannot be used with Internet Fax or Mail to Print.

Press [Memory Lock Reception].

Select [On] or [Off], and then press [OK].

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search