ManualsContents
SettingsHelp

# Resending a File

Previous Next

Machine memory stores documents that could not be successfully transmitted using Memory Transmission. Use this procedure to resend these documents.

Set "Store documents in memory that could not be transmitted" to "On" in User Parameter (switch 24, bit 0) in the Facsimile Features menu. See Parameter Settings.

Press [TX/RX Status / Print].

Press [Check / Stop Transmission File].

Select the file you want to resend.

`“TX failed”` is displayed for files that could not be sent.

If multiple destinations were specified, only the name of the destination you specify first and only the number of destinations that have not received the document you sent are shown.

Press [Transmit Failed File].

To add a destination, press [Add Destination], and then specify the destination.

Press [OK].

Repeat from step 3 to resend another file.

Press [Exit] twice.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search