ManualsContents
SettingsHelp

# Edit

Previous Next

This section describes the user tools in the Edit menu under [Copier / Document Server Features].

Enter the width of the binding margin with the number keys as follows:

- (mainly Europe and Asia)

  0–30 mm (in increments of 1 mm)

- (mainly North America)

  0.0–1.2 inches (in increments of 0.1 inches)

Enter the width of the erased margin with the number keys as follows:

- (mainly Europe and Asia)

  2–99 mm (in increments of 1 mm)

- (mainly North America)

  0.1–3.9 inches (in increments of 0.1 inches)

An image of approximately 1.5 mm (0.06 inches) will not be displayed as the width of the separation line, when specifying solid or broken lines.

Front Margin: Left / Right

Specify left and right margins on the front side of copies in Margin Adjustment mode.

Default:

(mainly Europe and Asia)

[Left: 5 mm]

(mainly North America)

[Left: 0.2 inch]

Back Margin: Left / Right

Specify left and right margins on the back side of copies in Margin Adjustment mode.

Default:

(mainly Europe and Asia)

[Right: 5 mm]

(mainly North America)

[Right: 0.2 inch]

Front Margin: Top / Bottom

Specify top and bottom margins on the front side of copies in Margin Adjustment mode.

Default:

(mainly Europe and Asia)

[T / B: 0 mm]

(mainly North America)

[T / B: 0.0 inch]

Back Margin: Top / Bottom

Specify top and bottom margins on the back side of copies in Margin Adjustment mode.

Default:

(mainly Europe and Asia)

[T / B: 0 mm]

(mainly North America)

[T / B: 0.0 inch]

1 Sided 2 Sided Auto Margin: TtoT

In 1 Sided 2 Sided mode, you can specify the margins on the back side.

Default:

(mainly Europe and Asia)

[Right: 5 mm]

(mainly North America)

[Right: 0.2 inch]

1 Sided 2 Sided Auto Margin: TtoB

In 1 Sided 2 Sided mode, you can specify the margins on the back side.

Default:

(mainly Europe and Asia)

[T / B: 0 mm]

(mainly North America)

[T / B: 0.0 inch]

Erase Border Width

Specify the width for erasing border.

Default:

(mainly Europe and Asia)

[10 mm]

(mainly North America)

[0.4 inch]

Erase Original Shadow in Combine

In Combine mode, you can specify whether to erase a 3 mm, 0.1 inches boundary margin around all four edges of each original.

Default: [On]

Erase Centre Width

Specify the width of the erased center margins with this function.

Default:

(mainly Europe and Asia)

[10 mm]

(mainly North America)

[0.4 inch]

Front Cover Copy in Combine

You can make a combined copy on the front cover sheet when you select Front Cover mode.

- Combine

- Do not Combine

Default: [Combine]

Copy Order in Combine

You can select the copy order in Combine mode from [From Left to Right] or [From Top to Bottom].

- From Left to Right

- From Top to Bottom

Default: [From Left to Right]

Orientation: Booklet, Magazine

Select the opening orientation of copies made using Booklet or Magazine mode.

Default: [Open to Left]

Copy on Designating Page in Combine

Specify whether to make a combined copy on the inserted slip sheets in Designate / Chapter mode.

Default: [Combine]

Image Repeat Separation Line

You can select a separation line using the Image Repeat function from: [None], [Solid], [Broken A], [Broken B], or [Crop Marks].

Default for [Type of Separation Line]: [None]

In full color, you can also select the color of the separation line.

Default for [Colour of Separation Line in Full Colour]: [Black]

Separation line color cannot be specified when selecting [None].

In black and white, printing will be done in black.

Selecting solid or broken lines might produce a blank area of approximately 1.5 mm (0.06 inches) in width along the separation line.

Double Copies Separation Line

You can select a separation line using the Double Copies function from: [None], [Solid], [Broken A], [Broken B], or [Crop Marks].

Default for [Type of Separation Line]: [None]

In full color, you can also select the color of the separation line.

Default for [Colour of Separation Line in Full Colour]: [Black]

Separation line color cannot be specified when selecting [None].

In black and white, printing will be done in black.

Selecting solid or broken lines might produce a blank area of approximately 1.5 mm (0.06 inches) in width along the separation line.

Separation Line in Combine

You can select a separation line using the Combine function from: [None], [Solid], [Broken A], [Broken B], or [Crop Marks].

Default for [Type of Separation Line]: [None]

In full color, you can also select the color of the separation line.

Default for [Colour of Separation Line in Full Colour]: [Black]

Separation line color cannot be specified when selecting [None].

In black and white, printing will be done in black.

Selecting solid or broken lines might produce a blank area of approximately 1.5 mm (0.06 inches) in width along the separation line.

- For details about how to change the Copier / Document Server Features, see "Changing Default Settings", Connecting the Machine/ System Settings.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search