ManualsContents
SettingsHelp

# Specifications Required for the Internet Fax Destination Machines

Previous Next

This section explains the specifications required for the Internet Fax destination machine.

When communicating with full mode-compatible machines, you can take advantage of higher specifications for coding, original size, and resolution. For details about the specifications available in full mode, see "Internet Fax Transmission and Reception", Maintenance and Specifications.

Communication protocols

- Transmission

  SMTP

- Reception

  POP3, SMTP, IMAP4

E-mail format

- Format

  MIME, Base64

- Content-Type

  Image/tiff

  Multipart/mixed (text/plain, Image/tiff (attached file forms))

Data format

- Profile

  TIFF Profile S

- Coding

  MH

- Original size

  A4

- Resolution (dpi)

  200 × 100/200 × 200, 204 × 98/204 × 196

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search