ManualsContents
SettingsHelp

# hostname

Previous Next

Use the "hostname" command to change the printer name.

View settings

`msh> hostname`

IPv4 Configuration

`msh> hostname "interface_name" "printer_name"`

- Enter the printer name using up to 63 alphanumeric characters.

- You cannot use a printer name beginning "RNP" (in either upper or lower case).

- The Ethernet interface and IEEE 802.11 interface will have the same printer name.

- wlan can be specified only when the IEEE 802.11 interface is installed.

- If you do not specify an interface, the Ethernet interface is selected automatically.

Interface name | Interface configured
--- | ---
ether | Ethernet interface
wlan | IEEE 802.11 interface

Initializing the printer name for each interface

`msh>hostname "interface_name" clear name`

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search