ManualsContents
SettingsHelp

# wsmfp

Previous Next

Use the "wsmfp" command to view and configure the WSD (Device), WSD (Printer), WSD (Scanner) and SSL settings.

View settings

`msh> wsmfp`

Comment settings

`msh> wsmfp comments "comment"`

- If you do not specify a comment, the current setting is displayed.

Location configuration

`mah> wsmfp location "location"`

- If you do not specify a comment, the current setting is displayed.

Presentation URL configuration

`msh> wsmfp url "URL"`

- Enter the URL string in the "URL".

WSD (Device) TCP port configuration

`msh> wsmfp devport "port_number"`

- The Default is 53000.

WSD (Printer) TCP port configuration

`msh> wsmfp prnport "port_number"`

- The Default is 53001.

WSD (Printer) timeout configuration

`msh> wsmfp prntimeout [30-65535]`

- The default is 900 seconds.

WSD (Scanner) TCP port configuration

`msh> wsmfp scnport "port_number"`

- The Default is 53002.

SSL configuration

`msh> wsmfp ssl {on|off}`

Comment initialization

`msh> wsmfp clear comments`

Location initialization

`msh> wsmfp clear location`

Presentation URL initialization

`msh> wsmfp clear url`

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search