ManualsContents
SettingsHelp

# bonjour

Previous Next

Use the "bonjour" command to display bonjour-related settings.

View settings

Bonjour settings are displayed.

`msh> bonjour`

Bonjour service name setting

You can specify the bonjour service name.

`msh> bonjour cname "computer name"`

- The computer name can be entered using up to 63 alphanumeric characters.

- If you do not specify a character string, the current setting is displayed.

Bonjour Installation location information setting

You can enter information about the location where the printer is installed.

`msh> bonjour location "location"`

- Information about the location can be entered using up to 32 alphanumeric characters.

- If you do not specify a character string, the current setting is displayed.

Setting order of priority for each protocol

- msh> bonjour diprint [0-99]

- msh> bonjour lpr [0-99]

- msh> bonjour ipp [0-99]

You can specify the order of priority for "diprint", "lpr", and "ipp". Smaller numbers indicate higher priority.

IP TTL setting

`msh> bonjour ipttl [1-255]`

You can specify the IP TTL (the number of routers a packet can pass through).

- The default is 255.

Resetting the computer name and location information

You can reset the computer name and location information.

`msh> bonjour clear {cname|location}`

- cname: Reset the computer name. The default computer name will be displayed when the computer is restarted.

- location: Reset the location information. The previous location information will be deleted.

Interface configuration

`msh> bonjour linklocal "interface_name"`

- If you do not specify an interface, the Ethernet interface is selected automatically.

- If many types of interface are installed, configure the interface that communicates with linklocal address.

- If you do not specify an interface, the Ethernet interface is automatically selected.

- wlan can be specified only when the IEEE 802.11 interface is installed.

Interface | Interface configured
--- | ---
ether | Ethernet interface
wlan | IEEE 802.11 interface

Setting IPP-SSL printing

`msh> bonjour ippport {ipp|ssl}`

- If IPP-SSL printing is set to {ssl}, the IPP port number will appear as 443, and IPP-SSL printing can be performed with higher security.

- If IPP-SSL printing is set to {ipp}, the IPP port number will appear as 631. Port 631 is the port for normal IPP printing.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search