ManualsContents
SettingsHelp

# Printer Configuration

Previous Next

You can check the printer configuration using telnet.

This section explains the checking procedure for input/output trays and printer language.

- UNIX: Use the "info" parameter and the "rsh", "rcp", "ftp", and "sftp" commands. "rsh" and "rcp" cannot be used in a Windows environment.

- telnet: Use the "info" command.

Input Tray
Item | Description
--- | ---
No. | ID number of the paper tray
Name | Name of the paper tray
Paper Size | Size of paper loaded in the paper tray
Status | Current status of the paper tray Normal: Normal NoInputTray: No tray PaperEnd: No paper

Output Tray
Item | Description
--- | ---
No. | ID number of the output tray
Name | Name of the output tray
Status | Current status of the output tray Normal: Normal PaperExist: Paper exists OverFlow: Paper is full Error: Other errors

Printer Language
Item | Description
--- | ---
No. | ID number of the printer language used by the machine
Name | Name of the printer language used in the machine
Version | Version of the printer language

- For details about UNIX commands and parameters, see UNIX Supplement.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search