ManualsContents
SettingsHelp

# Adjusting the Volume

Previous Next

You can change the volume of the following sounds that the machine makes.

On Hook Mode

Heard when [On Hook] is pressed.

At Transmission

Heard when "Immediate Transmission" is performed.

At Reception

Heard when the machine receives a document.

At Dialing

Heard after pressing the [Start] key, until the line connects to the destination.

At Printing

Heard when a received document is printed.

Press the [User Tools / Counter] key.

Press [Facsimile Features].

Check that [General Settings] screen appears.

Press [Adjust Sound Volume].

Press [Lower] or [Louder] to adjust the volume, and then press [OK].

You can hear the actual volume by pressing [Check].

You can set the volume level to between 0 and 7.

Press the [User Tools / Counter] key.

- You can adjust the On Hook volume when you press [On Hook]. For details about how to adjust the On Hook volume, see "On Hook Dial", Fax.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search