ManualsContents
SettingsHelp

# dhcp6

Previous Next

Use the "dhcp6"command to display or configure DHCPv6 settings.

View settings

The following command displays the current DHCPv6 settings.

`msh> dhcp6`

DHCPv6 configuration and display

`msh> dhcp6 {ether|wlan} {on|off}`

Viewing and specifying operation mode for parameter acquisition

`msh> dhcp6 mode {router|dhcpv6|dhcpv6lite}`

Viewing and specifying the ID for the IPv6 address

`msh> dhcp6 iaid {0-4294967295}`

- A value entered here ranges from 0 to 4294967295.

Viewing and specifying RFC compliant/noncompliant domain name

`msh> dhcp6 encode rfc {on|off}`

Viewing and specifying DNS server address selection (obtained from the dhcpv6 server/user specified value)

`msh> dhcp6 dnsaddr {dhcp|static}`

DUID (DHCP unique ID) deletion and display

`msh> dhcp6 duid {clear}`

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search