ManualsContents
SettingsHelp

# Placing Originals

Previous Next

How to place originals

Place the original on the exposure glass or in the ADF.

- Placing originals on the exposure glass

  See Paper Specifications and Adding Paper for details.

- Placing originals in the ADF

  See Paper Specifications and Adding Paper for details.

Orientation in which you should place the originals

Place originals in the landscape orientation () if the size of the original is A4 or 81/2 × 11 or larger.

Place originals in the portrait orientation () if the size of the original is smaller than A4 or 81/2 × 11.

Original size | Placing on the exposure glass | Placing in the ADF
--- | --- | ---
A4, B4 JIS, A3, 81/2 × 11, 81/2 × 14, 11 × 17 |  |
B5 JIS, A5, 51/2 × 81/2 |  |

Recommended types of originals

For details about sizes of originals that you can place on the exposure glass or in the ADF and sizes that the machine can detect automatically, see "Recommended Original Sizes and Weights" and "Sizes Detectable with Auto Paper Select", Paper Specifications and Adding Paper.

- When sending a fax, the image output at the other end depends on the size and orientation of paper used in the receiver's machine. If the receiver does not use paper of the same size and orientation as that of the original, the fax image may be reduced in size, trimmed at both edges, or divided across two or more sheets. When sending an important original, ask the receiver about the size and orientation of the paper in their machine.

- An original of irregular (i.e. custom) size originals are scanned as regular size originals, so the receiver may find extra blank margins or edges of images missing. When sending a custom size or part of a large original, you can specify the scan area precisely. If you specify a scan area, only that area is scanned regardless of the actual size of the original. For details about specifying the scan area, see Scan Size.

- Documents of 800 mm (32 inches) or more in length must be sent by Memory Transmission. Immediate Transmission might not be possible depending on the resolution setting and the other party's machine's settings.

- If an original jams, press the [Stop] key, and then carefully remove the original.

- Generally, place A4, 81/2 × 11 originals in the landscape orientation (). If you place an A4, 81/2 × 11 original in the portrait orientation (), the image is sent rotated by 90 degrees. See Transmission with Image Rotation.

- You can send the first page from the exposure glass then the remaining pages from the ADF. You cannot change from the ADF to the exposure glass.

- When using the Internet Fax function, originals are sent at A4 size. Originals larger than A4 are reduced to A4 size. If the receiver's machine is compliant with the T.37 full mode, originals are sent at the size specified in the Address Book. See T.37 full mode.

- There may be a difference in the size of the image when it is printed at the destination.

- If the receiver uses paper of a smaller width than the original, the image is reduced to fit that paper. See Auto Reduce.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search