ManualsContents
SettingsHelp

# Missing Image Area

Previous Next

Even if you place originals in the ADF or on the exposure glass correctly, margin of a few millimeters on all four sides of the original might not be copied.

Missing Image Area

1. Leading edge: 4.2 ± 1.5 mm (0.17 ± 0.06 inches)

2. Trailing edge: 0.5–6.0 mm (0.02–0.24 inches) (3.0–6.0 mm (0.12–0.24 inches) in Duplex mode)

3. Left edge: 0.5–4.0 mm (0.02–0.16 inches)

4. Right edge: 0.5–4.0 mm (0.02–0.16 inches)

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search