ManualsContents
SettingsHelp

# Logging in using a LAN-Fax driver

Previous Next

Open the printer properties dialog box, and then click the [Advanced Options] tab.

Select the [General user authentication] check box.

If you want to encrypt the login password, enter the driver encryption key set on the machine.

If you do not want to encrypt the password, proceed to step 4.

Click [OK] to close the printer properties dialog box.

Open the document you want to send from an application.

Select [LAN-Fax] as the printer and then start the print job.

The [LAN-Fax] dialog box appears

Click [User Settings...].

Enter the login user name and login password already set on the machine or server for user authentication.

If you enter an invalid login user name and login password, sending and/or printing does not start.

Click [OK] to close the dialog box.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search