ManualsContents
SettingsHelp

# Margin Adjustment

Previous Next

Copies originals leaving a binding margin.

Press [Edit / Colour].

Make sure that [Margin Adj.] is selected. If [Margin Adj.] is not selected, press [Margin Adj.].

Specify a binding margin for the front side pages.

Specify a binding margin for the back side pages.

Margin on the back side of the page is valid when [1 Sided 2 Sided] or [Combine 2 Sides] is selected.

If you do not need to specify the margins for the back side pages, proceed to step 5.

Press [OK].

- You can specify the binding margin up to 30 mm (1.2 inches) in 1 mm (0.1 inches) increments.

- Press [] and [] to specify the top or bottom position. Press [] and [] to specify the left or right position.

- If you specify a binding margin that is too wide, part of the image may not be copied.

- When making copies in Combine mode, the binding margin is added to the copies after the combination is finished.

- You can change the settings for Margin Adjustment under [Edit] in User Tools. For details, see Edit.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search