ManualsContents
SettingsHelp

# netware

Previous Next

Use the "netware" command to view and configure the NetWare settings such as the print server name or file server name. The following commands are available only when an optional NetWare unit is installed.

NetWare Print Server Names

`msh> netware pname "character string"`

- Enter the NetWare print server name using up to 47 characters.

NetWare File Server Names

`msh> netware fname "character string"`

- Enter the NetWare file server name using up to 47 characters.

Encap type

`msh> netware encap {802.3|802.2|snap|ethernet2|auto}`

Remote Printer Number

`msh> netware rnum [0-254]`

- The default is 0.

Timeout

`msh> netware timeout [3-255]`

- The default is 15.

Print server mode

`msh> netware mode pserver`

`msh> netware mode ps`

Remote printer mode

`msh> netware mode rprinter`

`msh> netware mode rp`

NDS context name

`msh> netware context "character string"`

SAP interval

`msh> netware sap_interval [0-3600]`

It can be entered between 0 and 3600 seconds.

Setting login mode for file server

`msh> netware login server`

Setting login mode for NDS tree

`msh> netware login tree`

Setting login mode for NDS tree name

`msh> netware tree "NDS tree name"`

File transfer protocol

`msh> netware trans {ipv4pri|ipxpri|ipv4|ipx}`

- If you do not specify the protocol, the current setting is displayed.

Protocol | Set Protocol
--- | ---
ipv4pri | IPv4+IPX(IPv4)
ipxpri | IPv4+IPX(IPX)
ipv4 | IPv4
ipx | IPX

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search