ManualsContents
SettingsHelp

# Functions Available on the Fax's Initial Display for Remote Fax

Previous Next

You can specify the following items for the initial display on the client-side machine:

Memory Transmission, Original Type, Resolution, Scan Size, Mixed Original Sizes, Auto Density, Manual Density, Original Orientation, Original Settings, Stamp, Prg. Dest. (Program Destination), Select Line, Fax Header Print, Check / Stop Transmission File, Transmission File Status, Reception File Status, TX Status Report

- The machine supports the functions, transmission capability, reception capability, and available paper size of the remote machine equipped with a facsimile function. Otherwise, the functions that the remote machine does not have are not available.

- You can select the same G3 line as the remote machine.

- You can select one of two fax headers.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search