ManualsContents
SettingsHelp

# Specifications for Wireless LAN Board

Previous Next

Transmission spec.:

- (mainly Europe and Asia)

  - Based on IEEE 802.11a/b/g (wireless LAN)

  - Based on IEEE 802.11b/g (wireless LAN)

- (mainly North America)

  - Based on IEEE 802.11a/b/g (wireless LAN)

Protocol:

TCP/IP, IPX/SPX

Transmission Rate:

Auto select from the following speed:

1 Mbps, 2 Mbps, 5.5 Mbps, 6 Mbps, 9 Mbps, 11 Mbps, 12Mbps, 18Mbps, 24 Mbps, 36 Mbps, 48 Mbps, 54 Mbps

Frequency range (Center Frequency):

- (mainly Europe and Asia)

  - IEEE 802.11a/b/g wireless LAN:

    - 2412–2472 MHz (1–13 channels)

    - 5180–5320 MHz (36, 40, 44, 48, 52, 56, 60, and 64 channels)

  - IEEE 802.11b/g wireless LAN:

    - 2412–2462 MHz (1–11 channels)

- (mainly North America)

  - IEEE 802.11a/b/g wireless LAN:

    - 2412–2462 MHz (1–11 channels)

    - 5180–5320 MHz (36, 40, 44, 48, 52, 56, 60, and 64 channels)

Transmission mode:

- Ad hoc mode

- Infrastructure mode

- Web Image Monitor is supported.

- The channel in use might differ depending on the country.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search