ManualsContents
SettingsHelp

# Folder transmission

Previous Next

Values of Set Items for Scan to Folder

Item | Maximum value | Comments
--- | --- | ---
Number of path name characters on SMB | 256 alphanumeric characters | -
Number of user name characters on SMB | 128 alphanumeric characters | -
Number of password characters on SMB | 128 alphanumeric characters | -
Number of server name characters on FTP | 64 alphanumeric characters | -
Number of path name characters on FTP | 256 alphanumeric characters | -
Number of user name characters on FTP | 64 alphanumeric characters | -
Number of password characters on FTP | 64 alphanumeric characters | -
Number of path name characters on NCP | 256 alphanumeric characters | -
Number of user name characters on NCP | 128 alphanumeric characters | -
Number of password characters on NCP | 64 alphanumeric characters | -
Number of addresses you can specify at the same time | 50 addresses | You can specify a maximum of 50 directly entered destinations.
Sendable file size | 2,000 MB per file | -

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search