ManualsContents
SettingsHelp

# Transmitting while Checking Connection to Destination (Immediate Transmission)

Previous Next

Using Immediate Transmission, you can send documents while checking the connection to the destination.

You can specify fax or IP-Fax destinations.

If you specify Internet Fax, e-mail, folder destinations, and group or multiple destinations, the transmission mode is automatically switched to Memory Transmission.

- It is recommended that you call the receivers and confirm with them when sending important documents.

Press the [Home] key on the top left of the control panel, and press the [Facsimile] icon on the [Home] screen.

Make sure "Ready" appears on the screen.

Press [Immed. TX].

Place the original into the ADF.

Select the scan settings you require.

For details about the scan settings, see Scan Settings.

Specify a destination.

If you make a mistake, press the [Clear] key, and then enter again.

For details about specifying a destination, see Specifying a Destination.

Press the [Start] key.

Related topics

Sending originals using the exposure glass (Immediate Transmission)
PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search