ManualsContents
SettingsHelp

# 8021x

Previous Next

Use "8021x" command to display IEEE 802.1x related information.

View settings

`msh> 8021x`

Configuration

`msh> 8021x "parameter"`

Parameter | Value configured
--- | ---
eap {tls|ttls|leap|peap} {chap|mschap|mschapv2|pap|md5|tls} | You can specify the EAP authentication type. tls: EAP-TLS (default) ttls: EAP-TTLS leap: LEAP peap: PEAP chap, mschap, mschapv2, pap, md5, and tls are settings for the phase 2 method, and one of these must be specified if EAP-TTLS or PEAP is selected. Do not make these settings when using other EAP authentication types. If you select EAP-TTLS, you can select chap, mschap, mschapv2, pap, or md5. If you select PEAP, you can select mschapv2 or tls.
username "character string" | You can specify the login user name for the Radius server. Usable characters: ASCII 0x20-0x7e (31 bytes). The default is blank.
username2 "character string" | You can specify the phase 2 username for EAP-TTLS/PEAP phase 2 authentication. Usable characters: ASCII 0x20-0x7e (31 bytes). The default is blank.
domain "character string" | You can specify the login domain name for the Radius server. The characters you can enter are ASCII 0x20-0x7e (64 bytes), but not "@" or "\". The default is blank.
password "character string" | You can specify the login password for the Radius server. Usable characters: ASCII 0x20-0x7e (128 bytes). The default is blank.
srvcert {on|off} | You can set the server certificate. The default is "off".
imca {on|off} | You can enable or disable the certificate when the intermediate certificate authority is present. The default is "off".
srvid "character string" | You can set the server ID and sub domain of the certificate server. Usable characters: ASCII 0x20-0x7e (128 bytes). The default is blank.
subdomain {on|off} | You can specify whether or not to permit access to the machine by users in subdomains use. The default is "off".
claer {a each command|all} | Returns the selected setting to its default value. If you specify "all", all settings will be restored to their default values. However, IEEE 802.1x Auth. status (enable or disable) for Ethernet and wireless LAN will not be initialized.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search