ManualsContents
SettingsHelp

# Specifications for Scanner

Previous Next

Type:

Full-color scanner

Scan method:

Flatbed scanning

Image sensor type:

CCD Image Sensor

Scan type:

Sheet, book, three-dimensional object

Original sizes that can be scanned:

- Length

  10–297 mm (0.4–11 inches)

- Width

  10–432 mm (0.4–17 inches)

Scan sizes automatically detectable from the exposure glass:

- (mainly Europe and Asia)

  A3, B4 JIS, A4, B5 JIS, A5, 81/2 × 13

- (mainly North America)

  11 × 17, 81/2 × 14, 81/2 × 11, 51/2 × 81/2

Scan sizes automatically detectable from the ADF:

- (mainly Europe and Asia)

  Types 1 and 2: A3, B4 JIS, A4, B5 JIS, A5, 11 × 17, 81/2 × 11, 81/2 × 13

  Types 3 and 4: A3, B4 JIS, A4, B5 JIS, A5, B6 JIS, 11 × 17, 81/2 × 11, 81/2 × 13

- (mainly North America)

  A3, A4, 11 × 17, 81/2 × 14, 81/2 × 11, 51/2 × 81/2, 10 × 14, 71/4 × 101/2

Scan speed (Types 1 and 2):

When using the E-mail, Scan to Folder, WSD (Push Type), Scan to Removable device, or network delivery scanner function (Original size: A4, Resolution: 200 dpi, one-side scanning):

- Black and white: 51 pages/minute

  (Original Type: B & W: Text / Line Art, Compression (Black & White): MH, ITU-T No1 Chart)

- Full Color: 51 pages/minute

  (Original Type: Full Colour: Text / Photo, Compression (Grey Scale / Full Colour): Default, Original Chart)

Scanning speed differs depending on the following; operating environment of the machine and computer, scan settings, and the content of originals (denser images require more time).

Scan speed (Types 3 and 4; models equipped with the ARDF):

When using the E-mail, Scan to Folder, WSD (Push Type), Scan to Removable device, or network delivery scanner function

(Original size: A4, Resolution: 200 dpi/300 dpi, one-side scanning):

- Black and white: 67 pages/minute

  (Original Type: B & W: Text / Line Art, Compression (Black & White): MH, ITU-T No1 Chart)

- Full Color: 67 pages/minute

  (Original Type: Full Colour: Text / Photo, Compression (Grey Scale / Full Colour): Default, Original Chart)

Scanning speed differs depending on the following; operating environment of the machine and computer, scan settings, and the content of originals (denser images require more time).

Scan speed (Types 3 and 4; models equipped with the one-pass duplex scanning ADF):

When using the E-mail, Scan to Folder, WSD (Push Type), Scan to Removable device, or network delivery scanner function

(Original size: A4, Resolution: 200 dpi/300 dpi, one-side scanning):

- Black and white: 85 pages/minute

  (Original Type: B & W: Text / Line Art, Compression (Black & White): MH, ITU-T No1 Chart)

- Full Color: 85 pages/minute

  (Original Type: Full Colour: Text / Photo, Compression (Grey Scale / Full Colour): Default, Original Chart)

Scanning speed differs depending on the following; operating environment of the machine and computer, scan settings, and the content of originals (denser images require more time).

Tone:

Black and white: 2 tones

Full color / Gray scale: 256 tones

Basic scanning resolution:

200 dpi

Image compression type for black and white (two-value) :

TIFF (MH, MR, MMR, JBIG2)

Image compression type for gray scale/full color:

JPEG

Interface:

Standard

- Ethernet interface (100BASE-TX/10BASE-T)

- USB 2.0 port (Type A)

- SD card slot

Option:

- Gigabit Ethernet interface (1000BASE-T/100BASE-TX/10BASE-T)

- IEEE 802.11a/b/g wireless LAN interface

Network protocol:

TCP/IP

Selectable scanning resolutions when using the E-mail function:

100 dpi, 200 dpi, 300 dpi, 400 dpi, 600 dpi

Protocol for sending e-mail:

SMTP

Sendable file formats when using the E-mail function:

TIFF, JPEG, PDF, High Compression PDF, PDF/A

When you select [PDF], [High Compression PDF], or [PDF/A] for the file format, you can attach a digital signature. You can also specify the security settings for [PDF] or [High Compression PDF]. For details, see "Specifying Digital Signature for PDF files", "Security Settings for PDF Files", Scan.

Selectable scanning resolutions when using the Scan to Folder function:

100 dpi, 200 dpi, 300 dpi, 400 dpi, 600 dpi

Protocol for Scan to Folder:

SMB, FTP, NCP

Sendable file formats when using the Scan to Folder function:

TIFF, JPEG, PDF, High Compression PDF, PDF/A

When you select [PDF], [High Compression PDF], or [PDF/A] for the file format, you can attach a digital signature. You can also specify the security settings for [PDF] or [High Compression PDF]. For details, see "Specifying Digital Signature for PDF files", "Security Settings for PDF Files", Scan.

Protocol for sending using WSD:

Web Services on Devices for scanning

Selectable scanning resolution when using TWAIN scanner:

100–1,200 dpi

Protocol for TWAIN scanner:

TCP/IP

Operating system for TWAIN scanner:

Windows XP/Vista/7, Windows Server 2003/2003 R2/2008/2008 R2

(TWAIN scanner runs in 32-bit compatible mode on a 64-bit operating system.)

Selectable scanning resolutions when using the network delivery scanner function:

100 dpi, 200 dpi, 300 dpi, 400 dpi, 600 dpi

Selectable scanning resolutions when using WIA scanner:

100–1,200 dpi

Protocol for WIA scanner:

TCP/IP

Operating system for WIA scanner:

Windows Vista (SP1 or later)/7, Windows Server 2008/2008 R2

(WIA scanner can function under both 32- and 64-bit operating systems.)

- Specifications are subject to change without notice.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search