ManualsContents
SettingsHelp

# Specifications for Bluetooth Interface Unit

Previous Next

Supported Versions

Bluetooth Version 2.0 + EDR

USB Interface

USB 1.1

Supported profiles

- SPP (Serial Port Profile)

- HCRP (Hardcopy Cable Replacement Profile)

- BIP (Basic Imaging Profile)

Frequency range

2400–2483.5 MHz

Transmission Method

Frequency Hopping Spread Spectrum (FHSS) Modulation

Transmission Speed

- Asynchronous Communication : Approximately 2.1 Mbps (Max)

- Synchronous Communication : Approximately 1.3 Mbps (Max)

- The transmission speed may vary depending on the factors such as the distance and obstacles between devices, radio wave condition, and Bluetooth devices being used.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search