ManualsContents
SettingsHelp

# Remote Transmission

Previous Next

Before the operation, confirm that the main power switch of the remote machine is turned on.

Press the [Home] key on the top left of the control panel.

Press the [Remote Fax] icon on the [Home] screen.

Place the original into the ADF or on the exposure glass.

Make the scan settings you require.

For details, see Scan Settings.

Specify a destination.

Press the [Start] key.

- For the following functions, use information stored or registered on the client-side machine:

  - Information registered in the Address Book

  - LDAP server settings

Related topics

Confirming Files in Memory of a Remote Fax
PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search